**1.2.2.2**

* Ingress port = port where frame is received from, frames are not forwarded to that port
* In a collision domain devices ‘compete’ for bandwidth. If two devices send a frame at the ssame time, a collision occurs.
* Hub always broadcasts to all ports, switch only to destination port (keeps record of MAC addresses)